Installation instructions
-------------------------

  To install RS Accuracy, follow these simple steps:

  1. Copy all of the distribution files to a location on 
     your hard drive (e.g. C:\temp).  
  2. Run the installer by double-clicking on the setup.exe icon.  
  3. Follow the instructions of the installer program to install the software.  
  4. Done! RS Accuracy should be installed on your system. 
